**How to use the toolflow:**

1. MIPS file:
   1. is used for adding of mars code to be used for testing
2. Src file:
   1. do not touch mem file
   2. put the MIPS processor into the MIPS\_Processor and use the signals that were provided can add additional ones if needed
   3. the tb is used for testing of the mips
   4. Add the components that you need into this file as well
3. Temp file:
   1. Used for the error output in each of the different .txt documents

**To run:**

Double click on the “RunTestFramework” another box will come up to compile everything then another box will come up and can click which mars program want to run.